Базовая настройка правил файрволла

Защита роутера MikroTik, базовые правила по настройке Firewall Вернуться назад

/ip firewall connection tracking set udp-timeout=10s /ip firewall filter add action=accept chain=input comment=\ "defconf: accept established,related,untracked" connection-state=\ established,related,untracked add action=drop chain=input comment="defconf: drop invalid" connection-state=\ invalid add action=accept chain=input comment="defconf: accept ICMP" protocol=icmp add action=accept chain=input comment=\ "defconf: accept to local loopback (for CAPsMAN)" dst-address=127.0.0.1 add action=drop chain=input comment="defconf: drop all not coming from LAN" \ in-interface-list=!LAN add action=accept chain=forward comment="defconf: accept in ipsec policy" \ ipsec-policy=in,ipsec add action=accept chain=forward comment="defconf: accept out ipsec policy" \ ipsec-policy=out,ipsec add action=fasttrack-connection chain=forward comment="defconf: fasttrack" \ connection-state=established,related hw-offload=yes add action=accept chain=forward comment=\ "defconf: accept established,related, untracked" connection-state=\ established,related,untracked add action=drop chain=forward comment="defconf: drop invalid" \ connection-state=invalid add action=drop chain=forward comment=\ "defconf: drop all from WAN not DSTNATed" connection-nat-state=!dstnat \ connection-state=new in-interface-list=WAN /ip firewall nat add action=masquerade chain=srcnat comment="defconf: masquerade" \ ipsec-policy=out,none out-interface-list=WAN