TL-SG2428P

configure # vlan 2 name "mgmt" # vlan 2000 name "VLAN2000" # # hostname 10.90.7.181 location "BACKUP" serial_port baud_rate 38400 contact-info helpdesk@link-region.ru # # system-time ntp UTC+03:00 10.90.7.1 10.90.7.1 12 no system-time dst # sdm prefer pca-default # jumbo-size 2022 # # dot1q-tunnel # # user name link privilege admin password 7 qwerty1234 no user name admin no service reset-disable # # # # pppoe id-insertion # # # snmp-server snmp-server community "lpublic" read-only "viewDefault" # # lldp # # # access-list packet-content profile chunk-offset0 3 chunk-offset1 4 chunk-offset2 5 chunk-offset3 6 access-list create 2001 access-list packet-content config 2001 rule 1 deny logging enable chunk0 00070000 mask0 00FF0000 access-list packet-content config 2001 rule 6 permit logging disable access-list create 1001 access-list combined 1001 rule 1 deny logging disable sip 192.168.0.0 sip-mask 255.255.0.0 access-list combined 1001 rule 6 deny logging disable sip 169.254.0.0 sip-mask 255.255.0.0 access-list combined 1001 rule 11 deny logging disable smac ff:ff:ff:ff:ff:ff smask ff:ff:ff:ff:ff:ff access-list combined 1001 rule 16 deny logging disable smac 00:00:00:00:00:00 smask ff:ff:ff:ff:ff:ff access-list combined 1001 rule 21 deny logging disable smac 00:00:00:00:00:00 smask ff:ff:ff:ff:ff:00 access-list create 1501 access-list ipv6 1501 rule 1 deny logging disable # access-list bind 2001 interface gigabitEthernet 1/0/1-23 access-list bind 1501 interface gigabitEthernet 1/0/1-23 access-list bind 1001 interface gigabitEthernet 1/0/1-23 # loopback-detection loopback-detection recovery-time 300 # # # # no controller cloud-based interface vlan 1 no ip address ipv6 enable shutdown # interface vlan 2 ip address 10.90.7.181 255.255.255.0 no ipv6 enable # # # # interface range gigabitEthernet 1/0/1-23 switchport general allowed vlan 2000 untagged no switchport general allowed vlan 1 switchport pvid 2000 storm-control broadcast 64 storm-control exceed shutdown recover-time 300 ip dhcp filter no ip igmp snooping no lldp receive no lldp transmit loopback-detection config process-mode port-based recovery-mode auto loopback-detection # # # interface gigabitEthernet 1/0/24 switchport general allowed vlan 2,2000 tagged switchport acceptable frame tagged no switchport general allowed vlan 1 vlan_trunk no ip igmp snooping lldp snmp-trap lldp management-address 10.90.7.181 # # # interface range ten-gigabitEthernet 1/0/25-26 switchport general allowed vlan 2,2000 tagged switchport acceptable frame tagged no switchport general allowed vlan 1 vlan_trunk speed 1000 no ip igmp snooping lldp snmp-trap lldp management-address 10.90.7.181 # # interface range ten-gigabitEthernet 1/0/27-28 switchport general allowed vlan 2,2000 tagged switchport acceptable frame tagged no switchport general allowed vlan 1 vlan_trunk no ip igmp snooping lldp snmp-trap lldp management-address 10.90.7.181